0 / 8 1 / 9 2 / A 3 / B 4 / C 5 / D 6 / E 7 / F

F8 F0 E8 E0 D8 D0 C8 C0 B8 B0 A8 A0 98 90 88 80 78 70 68 60 58 50 48 40 38 30 28 20 18 10 8 0 CLTS,

XLAT,

LEAVE,

ENTER,

PUSHI|B,

PUSHI|X,

POP|GS,

PUSH|GS,

CPUID,

POP|FS,

PUSH|FS,

AS:,

OS:,

GS:,

FS:,

POP|ALL,

PUSH|ALL,

STD,

CLD,

STI,

CLI,

STC,

CLC,

CMC,

HLT,

REPZ,

REPNZ,

LOCK,

IRET,

INTO,

INT3,

RETFAR,

RET,

LAHF,

SAHF,

POPF,

PUSHF,

WAIT,

CWD,

CBW,

AAS,

AAA,

DAS,

DAA,

DS:,

SS:,

CS:,

ES:,

JCXZ,

LOOP,

LOOPZ,

LOOPNZ, JMPS,

JMP,

CALL,

RETFAR+,

RET+,

JMPFAR,

CALLFAR,

INT, AAD,

AAM,

POP|DS,

POP|SS,

POP|ES,

PUSH|DS,

PUSH|SS,

PUSH|CS,

PUSH|ES, SET,

J|X,

MOV|CD,

SARI, SARI,

SHRI, SHRI,

SHLI, SHLI,

RCRI, RCRI,

RCLI, RCLI,

RORI, RORI,

ROLI, ROLI,

SAR, SAR, SAR, SAR,

SHR, SHR, SHR, SHR,

SHL, SHL, SHL, SHL,

RCR, RCR, RCR, RCR,

RCL, RCL, RCL, RCL,

ROR, ROR, ROR, ROR,

ROL, ROL, ROL, ROL,

MOV|SG, MOV|SG,

J, J, J, J, J, J, J, J, J, J, J, J, J, J, J, J,

OUTS, OUTS,

INS, INS,

OUT|D, OUT|D,

IN|D, IN|D,

OUT|P, OUT|P,

IN|P, IN|P,

SCAS, SCAS,

LODS, LODS,

STOS, STOS,

CMPS, CMPS,

MOVS, MOVS, TESTI|A, TESTI|A,

CMPI|A, CMPI|A,

XORI|A, XORI|A,

SUBI|A, SUBI|A,

ANDI|A, ANDI|A,

SBBI|A, SBBI|A,

ADCI|A, ADCI|A,

ORI|A, ORI|A,

ADDI|A, ADDI|A,

MOV|FA, MOV|FA,

MOV|TA, MOV|TA,

LMSW,

SMSW,

LIDT,

LGDT,

SIDT,

SGDT,

VERW,

VERR,

LTR,

LLDT,

STR,

SLDT,

BTCI,

BTRI,

BTSI,

BTI,

JMPFARO,

CALLFARO,

JMPO,

CALLO,

PUSH,

POP,

TESTI, TESTI, DEC, DEC,

INC, INC,

IDIV|AD, IDIV|AD,

DIV|AD, DIV|AD,

IMUL|AD, IMUL|AD,

MUL|AD, MUL|AD,

NEG, NEG,

NOT, NOT,

CMPSI,

SUBSI,

SBBSI,

ADCSI,

ADDSI,

CMPI, CMPI,

XORI, XORI,

SUBI, SUBI,

ANDI, ANDI,

SBBI, SBBI,

ADCI, ADCI,

ORI, ORI,

ADDI, ADDI,

MOVI|XR, MOVI|XR, MOVI|XR, MOVI|XR, MOVI|XR, MOVI|XR, MOVI|XR, MOVI|XR,

MOVI|BR, MOVI|BR, MOVI|BR, MOVI|BR, MOVI|BR, MOVI|BR, MOVI|BR, MOVI|BR,

XCHG|AX,XCHG|AX,XCHG|AX,XCHG|AX,XCHG|AX,XCHG|AX,XCHG|AX,XCHG|AX,

POP|X, POP|X, POP|X, POP|X, POP|X, POP|X, POP|X, POP|X,

PUSH|X, PUSH|X, PUSH|X, PUSH|X, PUSH|X, PUSH|X, PUSH|X, PUSH|X,

DEC|X, DEC|X, DEC|X, DEC|X, DEC|X, DEC|X, DEC|X, DEC|X,

INC|X, INC|X, INC|X, INC|X, INC|X, INC|X, INC|X, INC|X,

MOVI, MOVI,

IMUL,

MOVSX|W,

MOVZX|W,

MOVSX|B,

MOVZX|B,

LGS,

LFS,

LSS,

SHRDI,

SHLDI,

BSR,

BSF,

SHRD|C,

SHLD|C,

BTC,

BTR,

BTS,

BT,

LSL,

LAR,

IMULSI,

IMULI,

ARPL,

BOUND,

LDS,

LES,

LEA,

MOV, MOV, MOV, MOV,

XCHG, XCHG,

TEST, TEST,

CMP, CMP, CMP, CMP,

XOR, XOR, XOR, XOR,

SUB, SUB, SUB, SUB,

AND, AND, AND, AND,

SBB, SBB, SBB, SBB,

ADC, ADC, ADC, ADC,

OR, OR, OR, OR,

ADD, ADD, ADD, ADD,

QUICK REFERENCE PAGE FOR 80386 ASSEMBLER

By Albert van der Horst DFW Holland